From 7808740e100ba30ffb791044f3b14dec3e85ed6f Mon Sep 17 00:00:00 2001
From: Markus Koschany <apo@debian.org>
Date: Tue, 21 Feb 2023 14:26:43 +0100
Subject: [PATCH] CVE-2023-0795

This is also the fix for CVE-2023-0796, CVE-2023-0797, CVE-2023-0798,
CVE-2023-0799.

Bug-Debian: https://bugs.debian.org/1031632
Origin: https://gitlab.com/libtiff/libtiff/-/commit/afaabc3e50d4e5d80a94143f7e3c997e7e410f68

Upstream-Status: Backport [import from debian http://security.debian.org/debian-security/pool/updates/main/t/tiff/tiff_4.1.0+git191117-2~deb10u7.debian.tar.xz ]
CVE: CVE-2023-0795 CVE-2023-0796 CVE-2023-0797 CVE-2023-0798 CVE-2023-0799
Signed-off-by: Chee Yang Lee <chee.yang.lee@intel.com>

Signed-off-by: Hitendra Prajapati <hprajapati@mvista.com>
---
 tools/tiffcrop.c | 51 ++++++++++++++++++++++++++++--------------------
 1 file changed, 30 insertions(+), 21 deletions(-)

diff --git a/tools/tiffcrop.c b/tools/tiffcrop.c
index adf0f84..deba170 100644
--- a/tools/tiffcrop.c
+++ b/tools/tiffcrop.c
@@ -269,7 +269,6 @@ struct  region {
   uint32_t width;     /* width in pixels */
   uint32_t length;    /* length in pixels */
   uint32_t buffsize;  /* size of buffer needed to hold the cropped region */
-  unsigned char *buffptr; /* address of start of the region */
 };
 
 /* Cropping parameters from command line and image data 
@@ -524,7 +523,7 @@ static int rotateContigSamples24bits(uint16_t, uint16_t, uint16_t, uint32_t,
 static int rotateContigSamples32bits(uint16_t, uint16_t, uint16_t, uint32_t,
                                      uint32_t, uint32_t, uint8_t *, uint8_t *);
 static int rotateImage(uint16_t, struct image_data *, uint32_t *, uint32_t *,
-                       unsigned char **);
+                       unsigned char **, int);
 static int mirrorImage(uint16_t, uint16_t, uint16_t, uint32_t, uint32_t,
                        unsigned char *);
 static int invertImage(uint16_t, uint16_t, uint16_t, uint32_t, uint32_t,
@@ -5219,7 +5218,6 @@ initCropMasks (struct crop_mask *cps)
      cps->regionlist[i].width = 0;
      cps->regionlist[i].length = 0;
      cps->regionlist[i].buffsize = 0;
-     cps->regionlist[i].buffptr = NULL;
      cps->zonelist[i].position = 0;
      cps->zonelist[i].total = 0;
      }
@@ -6511,8 +6509,13 @@ static int  correct_orientation(struct image_data *image, unsigned char **work_b
                  (uint16_t) (image->adjustments & ROTATE_ANY));
       return (-1);
       }
- 
-    if (rotateImage(rotation, image, &image->width, &image->length, work_buff_ptr))
+
+      /* Dummy variable in order not to switch two times the
+       * image->width,->length within rotateImage(),
+       * but switch xres, yres there. */
+      uint32_t width = image->width;
+      uint32_t length = image->length;
+      if (rotateImage(rotation, image, &width, &length, work_buff_ptr, TRUE))
       {
       TIFFError ("correct_orientation", "Unable to rotate image");
       return (-1);
@@ -6580,7 +6583,6 @@ extractCompositeRegions(struct image_data *image,  struct crop_mask *crop,
     /* These should not be needed for composite images */
     crop->regionlist[i].width = crop_width;
     crop->regionlist[i].length = crop_length;
-    crop->regionlist[i].buffptr = crop_buff;
 
     src_rowsize = ((img_width * bps * spp) + 7) / 8;
     dst_rowsize = (((crop_width * bps * count) + 7) / 8);
@@ -6817,7 +6819,6 @@ extractSeparateRegion(struct image_data *image,  struct crop_mask *crop,
 
   crop->regionlist[region].width = crop_width;
   crop->regionlist[region].length = crop_length;
-  crop->regionlist[region].buffptr = crop_buff;
 
   src = read_buff;
   dst = crop_buff;
@@ -7695,7 +7696,7 @@ processCropSelections(struct image_data *image, struct crop_mask *crop,
     if (crop->crop_mode & CROP_ROTATE) /* rotate should be last as it can reallocate the buffer */
       {
       if (rotateImage(crop->rotation, image, &crop->combined_width, 
-                      &crop->combined_length, &crop_buff))
+                      &crop->combined_length, &crop_buff, FALSE))
         {
         TIFFError("processCropSelections", 
                   "Failed to rotate composite regions by %"PRIu32" degrees", crop->rotation);
@@ -7805,7 +7806,7 @@ processCropSelections(struct image_data *image, struct crop_mask *crop,
            * ToDo: Therefore rotateImage() and its usage has to be reworked (e.g. like mirrorImage()) !!
            */
 	if (rotateImage(crop->rotation, image, &crop->regionlist[i].width, 
-			&crop->regionlist[i].length, &crop_buff))
+			&crop->regionlist[i].length, &crop_buff, FALSE))
           {
           TIFFError("processCropSelections", 
                     "Failed to rotate crop region by %"PRIu16" degrees", crop->rotation);
@@ -7937,7 +7938,7 @@ createCroppedImage(struct image_data *image, struct crop_mask *crop,
   if (crop->crop_mode & CROP_ROTATE) /* rotate should be last as it can reallocate the buffer */
     {
     if (rotateImage(crop->rotation, image, &crop->combined_width, 
-                    &crop->combined_length, crop_buff_ptr))
+                    &crop->combined_length, crop_buff_ptr, TRUE))
       {
       TIFFError("createCroppedImage", 
                 "Failed to rotate image or cropped selection by %"PRIu16" degrees", crop->rotation);
@@ -8600,7 +8601,7 @@ rotateContigSamples32bits(uint16_t rotation, uint16_t spp, uint16_t bps, uint32_
 /* Rotate an image by a multiple of 90 degrees clockwise */
 static int
 rotateImage(uint16_t rotation, struct image_data *image, uint32_t *img_width,
-            uint32_t *img_length, unsigned char **ibuff_ptr)
+            uint32_t *img_length, unsigned char **ibuff_ptr, int rot_image_params)
   {
   int      shift_width;
   uint32_t   bytes_per_pixel, bytes_per_sample;
@@ -8791,11 +8792,15 @@ rotateImage(uint16_t rotation, struct image_data *image, uint32_t *img_width,
 
               *img_width = length;
               *img_length = width;
-              image->width = length;
-              image->length = width;
-              res_temp = image->xres;
-              image->xres = image->yres;
-              image->yres = res_temp;
+            /* Only toggle image parameters if whole input image is rotated. */
+            if (rot_image_params)
+            {
+                image->width = length;
+                image->length = width;
+                res_temp = image->xres;
+                image->xres = image->yres;
+                image->yres = res_temp;
+            }
 	      break;
 
     case 270: if ((bps % 8) == 0) /* byte aligned data */
@@ -8868,11 +8873,15 @@ rotateImage(uint16_t rotation, struct image_data *image, uint32_t *img_width,
 
               *img_width = length;
               *img_length = width;
-              image->width = length;
-              image->length = width;
-              res_temp = image->xres;
-              image->xres = image->yres;
-              image->yres = res_temp;
+            /* Only toggle image parameters if whole input image is rotated. */
+            if (rot_image_params)
+            {
+                image->width = length;
+                image->length = width;
+                res_temp = image->xres;
+                image->xres = image->yres;
+                image->yres = res_temp;
+            }
               break;
     default:
               break;
-- 
2.25.1

