From 00ae1ee97ad3ad0624798b28c6bab94a19b3ef39 Mon Sep 17 00:00:00 2001
From: Zhenhua Luo <zhenhua.luo@nxp.com>
Date: Sat, 11 Jun 2016 22:08:29 -0500
Subject: [PATCH] fix the incorrect assembling for ppc wait mnemonic

The wait mnemonic for ppc targets is incorrectly assembled into 0x7c00003c due
to duplicated address definition with waitasec instruction. The issue causes
kernel boot calltrace for ppc targets when wait instruction is executed.

Upstream-Status: Pending
Signed-off-by: Zhenhua Luo <zhenhua.luo@nxp.com>
---
 opcodes/ppc-opc.c | 4 +---
 1 file changed, 1 insertion(+), 3 deletions(-)

diff --git a/opcodes/ppc-opc.c b/opcodes/ppc-opc.c
index a424dd924de..406d5b60917 100644
--- a/opcodes/ppc-opc.c
+++ b/opcodes/ppc-opc.c
@@ -6378,8 +6378,6 @@ const struct powerpc_opcode powerpc_opcodes[] = {
 {"waitasec",	X(31,30),      XRTRARB_MASK, POWER8,	POWER9,		{0}},
 {"waitrsv",	XWCPL(31,30,1,0),0xffffffff, POWER10,	EXT,		{0}},
 {"pause_short",	XWCPL(31,30,2,0),0xffffffff, POWER10,	EXT,		{0}},
-{"wait",	X(31,30),	XWCPL_MASK,  POWER10,	0,		{WC, PL}},
-{"wait",	X(31,30),	XWC_MASK,    POWER9,	POWER10,	{WC}},
 
 {"lwepx",	X(31,31),	X_MASK,	  E500MC|PPCA2, 0,		{RT, RA0, RB}},
 
@@ -6433,7 +6431,7 @@ const struct powerpc_opcode powerpc_opcodes[] = {
 
 {"waitrsv",	X(31,62)|(1<<21), 0xffffffff, E500MC|PPCA2, EXT,	{0}},
 {"waitimpl",	X(31,62)|(2<<21), 0xffffffff, E500MC|PPCA2, EXT,	{0}},
-{"wait",	X(31,62),	XWC_MASK,    E500MC|PPCA2, 0,		{WC}},
+{"wait",	X(31,62),	XWC_MASK,    E500MC|PPCA2|POWER9|POWER10, 0,	{WC}},
 
 {"dcbstep",	XRT(31,63,0),	XRT_MASK,    E500MC|PPCA2, 0,		{RA0, RB}},
 
