LICENSE = "CLOSED"

IMAGE_INSTALL:append = " linux-firmware-rpidistro-bcm43430 linux-firmware-bcm43455 bcm2835-dev"

# meta-raspberry specific configuration for raspberry pi devices
DISABLE_OVERSCAN = "1"
DISABLE_SPLASH = "1"
GPU_MEM = "64"
DISABLE_RPI_BOOT_LOGO = "1"
ENABLE_SPI_BUS = "1"

RPI_EXTRA_CONFIG = ' \n \
dtparam=spi=on \n \
dtparam=audio=on \n \
'