# crops-yocto

Full Yocto Linux build files for embedded linux devices with Flutter.
Contains a full example configuration for the Raspberry Pi 4 and Raspberry Pi Zero 2W.
Build the image, flash it to the sd and boot! ;)

Flutter-Pi and Flutter-Auto (Toyotas Flutter embedder) are supported.
Do not build the image with both selected.

The first build can take long (everything gets compiled from scratch for the embedded devices architecture).
First build on an AMD Ryzen 6800U: around 8 hours.

The build was only tested from a Linux device, but it uses docker to build.
It should also work on Windows via Docker.
An AMD64 CPU architecture is required. This will not work on Apple Silicon chips (for now).